    This disk contains VESA drivers VESA452.COM & VESA451.COM for
Chips and Technologies' 82C452 Super VGA and 82C451 VGA respectively,
and an utility SETVESA.EXE to change the paging configuration.

Usage:

     1. Install 452 VESA driver by executing VESA452.COM.

     2. Run VTEST.
